Aerophone Pro Gold Limited Edition(AE-30A) spec sheet

- Key Layout
Saxophone compatible

- Sound Generator
ZEN-Core
SuperNATURAL acoustic

- Parts
4 Parts (Drum: 1 Part)

- Preset Memory
Preset Scenes: more than 300

- User Memory
User Scenes: 600
Favorite Scenes: 12

- Effects
Multi-effects
Chorus
Delay
Reverb

- Controllers
Breath sensor
Bite sensor
Performance keys
Octave keys
Thumb lever
Thumb pad
S1/S2 button
SCENE buttons
MENU buttons
SCENE CATEGORY knob
TRANSPOSE knob
MIDI CONTROL switch
Motion sensor

- Bluetooth
Ver 4.2
Profile Support: A2DP (Audio), GATT (MIDI over Bluetooth Low Energy)
Codec: SBC (Support to the content protection of the SCMS-T method)

- Display
Graphic OLED 128 x 32 dots

- Connectors
PHONES jack: stereo miniature phone type
OUTPUT jack: stereo 1/4-inch phone type
MIDI (IN/OUT) connectors
USB COMPUTER/MEMORY port (USB Type-C(R) , AUDIO/MIDI)
DC IN jack

- External Memory
USB Flash drive (USB Type-C(R), commercially available)

- Speaker Amplifier Power Output
1.5 W x 2

- Speakers
2.8 cm x 2

- Power Supply
AC adaptor (DC 5.7 V)
Ni-MH battery (AA, HR6) (commercially available) x 6

- Current Draw
915 mA

- Battery life for continuous use (differs depending on the conditions of use)
Ni-MH batteries: approximately 6 hours (When using batteries having a capacity of 1,900 mAh.)

* Carbon-zinc or alkaline batteries cannot be used

- Dimensions
133 (W) x 84 (D) x 687 (H) mm
5-1/4 (W) x 3-5/16 (D) x 27-1/16 (H) inches

- Weight (including batteries)
1,140 g
2 lbs 9 oz

- Accessories
Owner's manual
Leaflet "USING THE UNIT SAFELY"
AC adaptor
Mouthpiece cap
Moisture band
USB cable (USB Type-C(R) - USB A)
Thumb hook cover (2 types)
Water basin
Dedicated hand carry bag emblazoned with the Aerophone 10th Anniversary logo 
Numbered certificate
Special letter from the Aerophone R&D team


- Options (sold separately)
Replacement Mouthpiece
(OP-AE05MPH)









●キー配列
サクソフォン互換キー配列

●音源
ZEN-Core
SuperNATURALアコースティック

●パート数
4パート（ドラムは1パート）

●プリセット・メモリー
プリセット・シーン：300以上

●ユーザー・メモリー
ユーザー・シーン：600
フェイバリット・シーン：12

●エフェクト
マルチ・エフェクト
コーラス
ディレイ
リバーブ

●コントローラー
ブレス・センサー
バイト・センサー
演奏キー
オクターブ・キー
サム・レバー
サム・パッド
S1/S2ボタン
SCENEボタン
MENUボタン
SCENE CATEGORYつまみ
TRANSPOSEつまみ
MIDI CONTROLスイッチ
モーション・センサー

●Bluetooth
標準規格Ver 4.2
対応プロファイル：A2DP（オーディオ）、GATT（MIDI over Bluetooth Low Energy）
対応コーデック：SBC（SCMS-T方式によるコンテンツ保護に対応）

●ディスプレイ
有機ELディスプレイ　128×32ドット

●接続端子
PHONES端子（ステレオ・ミニ・タイプ）
OUTPUT端子（ステレオ標準タイプ）
MIDI（IN／OUT）端子
USB COMPUTER/MEMORY端子（USB Type-C（R）、AUDIO／MIDI）
DC IN端子

●記憶メディア
USBメモリー（USB Type-C（R）、市販品）

●スピーカー・アンプ出力
1.5W×2

●スピーカー
2.8cm×2

●電源
ACアダプター（DC5.7V）
ニッケル水素電池（単3形）（市販品）×6

●消費電流
915mA

●連続使用時の電池の寿命（使用状態によって異なります）
ニッケル水素電池：約6時間（容量1,900mAh使用時）

※マンガン乾電池、アルカリ乾電池は使用不可

●外形寸法
133（幅）×84（奥行）×687（高さ）mm

●質量（電池含む）
1,140g

●付属品
取扱説明書
「安全上のご注意」チラシ
保証書
ACアダプター
マウスピース・キャップ
バンド
USBケーブル（USB Type-C（R） - USB A）
サム・フック・カバー（2タイプ）
ウォーター・プロテクター
Aerophone10周年記念ロゴ入り専用ハンド・キャリー・バッグ
シリアルナンバー入り認定証
Aerophone開発チームからのメッセージレター

●別売品
交換用マウスピース（OP-AE05MPH）

